|  |
| --- |
| **Synthetic Sling Inspection Record** |
| Manufacturer: | Model: | Serial Number: | Reach: | *Capacity:* |
| ***COMPONENT UNIT OR PART*** | ***PROBLEM*** | SAT | ADJ | REP | ***ACTION NOTES:***SAT=SATISFACTORYADJ=ADJUSTREP=REPAIR |
| Missing or illegible sling identification |  |  |  |  |  |
| Acid/caustic burns |  |  |  |  |  |
| Evidence of heat damage. |  |  |  |  |  |
| Holes, tears, cuts, abrasive wear or snags that expose the core yarns |  |  |  |  |  |
| Broken or damaged core yarns. |  |  |  |  |  |
| Weld splatter that exposes core yarns. |  |  |  |  |  |
| Knots in the round sling, except for core yarns inside the cover. |  |  |  |  |  |
| Fittings that are pitted, corroded, cracked, bent twisted, gouged, or broken. |  |  |  |  |  |
| Other conditions, including visible damage, that cause doubt as to the continued use of the sling |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |