08	MAINE OFFICE OF COMMUNITY AFFAIRS

004	MANUFACTURED HOUSING

Chapter 20	Used Standard - Body and Frame Requirement


SUMMARY:	The chapter of this rule is to assure that minimum requirements are met to provide structural strength and rigidity and protection against corrosion, decay, insects and other similar destructive forces.


Roof Loads

All homes manufactured prior to June 15, 1976, are exempt from meeting The National Manufactured Home Construction and Safety Standards for roof loads for the State of Maine, except:

1.	All homes with roofs added after construction will be inspected by a registered professional engineer to determine that the roof and home can withstand any snow loads or wind uplifts that may occur.

	Floors

All floors will be of a solid construction to protect users of the home from the hazard of an unsafe floor.

	Anchoring System

No park operator may require a manufactured home to be anchored unless a concrete slab is provided.

	Exterior Coverings

Exterior coverings shall be of moisture and weather resistant materials to resist wind, snow and rain.


EFFECTIVE DATE:		December 12, 1990

EFFECTIVE DATE (ELECTRONIC CONVERSION):	January 11, 1997

TRANSFER OF AUTHORITY TO ADMINISTER AND ENFORCE RULE: The authority to administer and enforce this rule (formerly 02-385 C.M.R. Ch. 930) was transferred to the Maine Office of Community Affairs on July 29, 2026 pursuant to PL 2025, c. 650, § RRR-58.
