
08	DEPARTMENT OF PROFESSIONAL AND FINANCIAL REGULATION

004	MANUFACTURED HOUSING 

Chapter 24	Used Standard - Electrical System


SUMMARY:	This chapter covers the electrical conductors and equipment installed within or on a home and the conductors that connect the home to the supply of electricity.


A person holding a master license issued by the State of Maine Electricians Examining Board shall inspect and certify that the electrical system that is accessible, including the wiring of the smoke detector, is safe and meets the National Electrical Code at the time the home was constructed.

A.	Homes wired with aluminum conductors shall meet the current Underwriter Laboratory (UL) requirements for connecting to branch circuits of 30 amps or less.  (Note:  The intent of this is not to require the home to be rewired but only to require that U. L. listed conductors be affixed to receptacle switches and light fixtures.  There are several methods of doing this.  The most preferred is the "pig tail" method.)


EFFECTIVE DATE:		December 12, 1990

EFFECTIVE DATE (ELECTRONIC CONVERSION):	January 11, 1997

TRANSFER OF AUTHORITY TO ADMINISTER AND ENFORCE RULE: The authority to administer and enforce this rule (formerly 02-385 C.M.R. Ch. 970) was transferred to the Maine Office of Community Affairs on July 29, 2026 pursuant to PL 2025, c. 650, § RRR-58.


