
Mr. MacDonald,


When you feel like trying these Drivers with your Office’s new plotter let me know. But in order to do that you will need to copy and move these two ptlcfg files to a folder on your local drive, C: I presume.

Make like you are going to Print:


MicroStation Dropdown Menu, **File > Print**, the Print Dialog Box comes up:



Now click on the “magnifying glass” near the center of the dialog box, another dialog box will come up:



Where ever this location / path is, put those two files here.



Now you should be able you use one of those drivers “full” for full size sheet (22x34) or the “half” for the half size sheet (11x17) when you print from MicroStation and it… should… look… pretty good maybe? This is DEFINITELY a work in progress so please feel free to tell me What You REALLY Think! I’m trying to get more information on how the whole plotting in MicroStation works and what adjustments can be made so hopefully the quality will improve with regards to the grayscale – at least.