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Chapter 21	Used Standard - Thermal Protection


SUMMARY:	This chapter outlines the minimum requirements for thermal protection.


Insulation

The minimum requirements for a home shall be as follows:

1.	Walls - R-11
2.	Roof - R-14
3.	Floor - R-11

A destructive inspection will not be performed to determine the actual amount, however, a thermal scan may be used to determine uniformity of the insulation.


EFFECTIVE DATE: December 12, 1990

EFFECTIVE DATE (ELECTRONIC CONVERSION):	January 11, 1997

TRANSFER OF AUTHORITY TO ADMINISTER AND ENFORCE RULE: The authority to administer and enforce this rule (formerly 02-385 C.M.R. Ch. 940) was transferred to the Maine Office of Community Affairs on July 29, 2026 pursuant to PL 2025, c. 650, § RRR-58.


